### Q1: In no more than three paragraphs, please describe the steps you took to setup remote connection. Using bullet points are much preferred.

* Using the Raspberry Pi with a Display, Mouse and Keyboard
  + In the Preferences Menu open the Raspberry Pi Configurator
  + Open the Interfaces Tab
  + Enable SSH
  + Click OK
  + Open Terminal and get the Pi’s IP Address using ‘ifconfig’
    - If the IP is issued using DHCP you should set a static IP
* On the client system
  + Install a suitable SSH client such as ‘Putty’ or another of your choice
  + Enter the IP Address of your Raspberry Pi in the ‘Hostname’ textbox
  + Check the port is correct, the SSH port is 22
  + Click connect
  + Authenticate using the Raspberry Pi Credentials
  + Start using the Raspberry Pi

### Q2: Paste the screen capture here and submit the file as your submission for task 6.1P.

